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AUTOMAZIONE ACCESS!
MADE IN ITALY




Series SIMPLY

Sliding gate automation. Up to 600 kg. 230 Vac/ 24 Vcc




 Features:
· Motor carcass in casting aluminum;
- Steel and cast iron gears;
- Mechanical parts lubricated with lithium grease against corrosion, oxidation and rust;
- Version with or without a control board;
- Control panel with radio receiver and antenna, in a special container with aerostop gasket against  insects and humidity;
- Easy wiring and easy software;
- High performance electric motor;
- Mechanical limit switch - magnetic switch - encoder (optional);
- Manual release lever with personalized key;
- Anti-crushing device (EN 12453);
- Loop torque control;
- Control panel with slowing down safety device (EN 12453);
- Extremely quiet ;
- Optional battery back-up kit;
· Power supply: 230 Vac/ 24 Vcc
Series CARRERA
Sliding gate automation. Up to 1000 kg. 230 Vac/ 24 Vcc



 

Features:
- Motor carcass in casting aluminum painted;
- Steel and cast iron gears;
- Mechanical parts lubricated with lithium grease against corrosion, oxidation and rust;
- Extremely quiet ;
- High performance electric motor;
- Manual release lever with personalized key;
- Mechanical limit switch - magnetic switch - encoder (optional);
- Loop torque control;
- Easy wiring and easy software;
- Version with or without a control board;
- Control panel with radio receiver and antenna, in a special container with aerostop gasket against insects and humidity;
- Anti-crushing device with reversing (EN 12453);
- Control panel with slowing down (EN 12453);
- Optional battery back-up kit

Series AG FUTURE
Sliding gate automation. Up to 1800 kg. 230 Vac



Features:
- Motor carcass in casting aluminum painted;
- Steel and cast iron gears; stator and the mechanical parts in oil bath
- except for the version to 800kg, is lubricated by grease;
- Oil level guard; 
- Version with or without a control board;
- Control panel with radio receiver and antenna, in a special container with aerostop gasket against  insects and humidity; 
- Easy wiring and easy software; 
- High performance electric motor; 
- Mechanical limit switch - magnetic switch (optional); 
- Manual release lever with personalized key;
- Loop torque control; 
- Extremely quiet ;
- Anti-crushing device with reversing (EN 12453); 
- Control panel with slowing down (EN 12453); 
- 1800kg three-phase version managed by a panel control inverter with "soft start-soft stop" function.

